{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Combustion","Engine","Bin"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[{"sheet":"Engine","index":1,"reason":"part_missing"},{"sheet":"Bin","index":2,"reason":"part_missing"}],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Combustion","index":0,"n_rows":31,"n_cols":12,"rows_kept":31,"cut":false,"hidden":false,"merged":[]}
["Gas Combustion Calculations"]
[]
["Basic Fuel Gas Chemical Compositions [% vol]"]
["Gas","Nitrogen","Hydrogen","Methane","Ethane","Propane","Carb. Mon.","Carb. Gas"]
[null,"N2","H2","CH4","C2H6","C3H8","CO","CO2"]
["Coke Oven",7.83,58.21,27.7,1.1499999999999999,0.28999999999999998,2.72,0.78]
["Natural",22.7,null,68.31,5.31,1.88,null,0.9]
[]
[null,"Butane","i-Butane","Benzene","Ethylene","Pentane","i-Pentane","Hydr. Sulf.",null,null,"                                                                                                                                                            "]
[null,"C4H10","i-C4H10","C6H6","C2H4","C5H12","i-C5H12","H2S"]
["GCO",0.06,0.05,0.1,1.03,null,null,0.09]
["GN",0.44,0.28000000000000003,",",null,0.08,0.11]
[]
["Assorted Data:",null,null,null,null,null,null,null,"Characteristics of the Resulting Fuel:"]
["Fuel Gas Mixture Flow Rate [Nm³/h]",null,null,1000,null,null,null,null,null,"Comp.","NHV","NHV"]
["Combustion Air Flow Rate [Nm³/h]",null,null,8055,null,null,null,null,null,"[% vol]","[Kcal/Nm³]","[%]"]
["COG Proportion in Fuel Mixture [%]",null,null,50,null,null,null,null,"Nitrogen",15.264999389648438]
["Air Relative Umidity [%]",null,null,60,null,null,null,null,"Carb. Gas",0.8399999737739563]
["Ambient Temperature [°C]",null,null,25,null,null,null,null,"Carb. Mon.",1.3600000143051147,41.058400431871419,0.69922332431060363]
["Fumes Temperature [°C]",null,null,470,null,null,null,null,"Hydrogen",29.104999542236328,751.49108818054196,12.797870626725761]
[null,null,null,null,null,null,null,null,"Methane",48.005001068115234,4107.7879413986202,69.955505079008702]
["Fumes Flow Rate and Chemical Composition",null,null,null,null,null,null,null,"Ethane",3.2300000190734863,492.12280290603644,8.3808365303462136]
[null,"CO2","H2O","N2","O2","SO2","Total",null,"Propane",1.0850000381469727,236.62765831947328,4.0297619033775494]
["[Nm³/h]",601.4063720703125,1564.8519287109375,6395.958984375,363.75723266601563,0.43745714426040649,8926.412109375,null,"Butane",0.25,70.98,1.2087872649086659]
["[% vol]",6.7373809814453125,17.530580520629883,71.652069091796875,4.0750665664672852,4.9007050693035126E-3,100,null,"i-Butane",0.16499999165534973,46.723047637045383,0.79569209582109601]
[null,null,null,null,null,null,null,null,"Pentane",3.9999999105930328E-2,13.977199687585236,0.23803129024286301]
["Assorted Results:",null,null,null,null,null,null,null,"i-Pentane",5.4999999701976776E-2,19.136699896305799,0.3258974235986678]
["Fuel Gas Mixture NHV [Kcal/m³]",null,null,5872.0009765625,null,null,null,null,"Ethylene",0.51499998569488525,72.697397980689999,1.2380345008601725]
["Theoretical Air:Fuel Ratio",null,null,6.3532142412094847,null,null,null,null,"Benzene",5.000000074505806E-2,16.911500252000987,0.28800234059056762]
["Combustion Heat [Mcal/h]",null,null,5708.3310546875,null,null,null,null,"Hydr. Sulf.",4.4999998062849045E-2,2.4871498929336671,4.2356087862738361E-2]
["Heat Lost to Fumes [Mcal/h]",null,null,1318.1776123046875]