{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Variable Data","Constant Data","Results"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Variable Data","index":0,"n_rows":27,"n_cols":9,"rows_kept":27,"cut":false,"hidden":false,"merged":[]}
["Variable Data for the Heat Balance of the Reheating Slab Furnace"]
[]
[]
["Identification:"]
["Date:"]
[]
[]
[null,"Fuel Gas","Air","Water","Water Exit","Air","Fumes","Stack Fumes","C.O.G."]
["Hour","Flowrate","Flowrate","Flowrate","Temper.","Temper.","Temper.","Temper.","Amount"]
["[hh:mm]","[Nm3/h]","[Nm3/h]","[Nm3/h]","[°C]","[°C]","[°C]","[°C]","[%]"]
["00:00:00"]
["00:30:00"]
["01:00:00"]
["01:30:00"]
["02:00:00"]
["02:30:00"]
["03:00:00"]
["03:30:00"]
["04:00:00"]
["04:30:00"]
["05:00:00"]
["05:30:00"]
["06:00:00"]
["06:30:00"]
["07:00:00"]
["07:30:00"]
["08:00:00"]

{"sheet":"Constant Data","index":1,"n_rows":23,"n_cols":9,"rows_kept":23,"cut":false,"hidden":false,"merged":[]}
[null,"Constant Data for the Heat Balance of the Reheating Slab Furnace"]
[]
[]
["Identification:"]
["Date:"]
[]
["Fuel Gases Chemical Composition [% vol]"]
[null,"N2","H2","CH4","C2H6","C3H8","CO","CO2","O2"]
["Coke Oven"]
["Natural Gas"]
[]
["External Wall Temperature [°C]",null,null,null,null,"Dados Diversos:"]
[null,"Pre-Heating","Heating","Soaking",null,"Air Relative Humidity [%]"]
["North",null,null,null,null,"Ambient Temperature [°C]"]
["South",null,null,null,null,"Slab Initial Temperature [°C]"]
["Roof",null,null,null,null,"Slab Final Temperature [°C]"]
["Hearth",null,null,null,null,"Cooling Water Initial Temp. [°C]"]
[null,null,null,null,null,"N2 Added to Natural Gas [%]"]
["Furnace Dimensions [m]",null,null,null,null,"Oxygen Amount in Fumes [%]"]
[null,"Pre-Heating","Heating","Soaking",null,"Scale Amount [%]"]
["Length",null,null,null,null,"Average Furnace Output [t/h]"]
["Height"]
["Width"]

{"sheet":"Results","index":2,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[]}
[null,"Results of the Heat Balance of the Reheating Slab Furnace"]
[]
["Identification:"]
["Date:"]
[]
["Heat Input"]
[null,null,null,"kcal/shift","kcal/kg steel","%"]
["Fuel Gas Combustion Heat"]
["Combustion Air Sensible Heat"]
["Scale Heat of Formation"]
["Slab Sensible Heat"]
["TOTAL"]
[]
["Heat Output"]
[null,null,null,"kcal/shift","kcal/kg steel","%"]
["Steel Enthalpy"]
["Fumes Enthalpy After Recuperator"]
["Cooling Water Enthalpy"]
["Furnace Wall Heat Loss"]
["Other Losses",null,null,null,null,null,"                                                                                                                                                                           "]
["TOTAL"]
[]
["Other Results"]
["Time Span for Analysis [h]"]